



Set 0x0F for Servo-On and then set 0x1F to start the homing